
------



**BQOCJS**

CELEBRATING

**1982-2022**



C

**Quality**

**A\_s\_s\_u\_r\_a\_n\_c\_e**

**40!**

**EQUUS SOPREMA COLPHENE BSW**

**Below-ground single layer waterproofing**

**Specification No: 4131EB Date Prepared: July 2024**

**Project & Address: Fisher & Paykel -Home & Shed Buildings**

**830 Great South Road, Penrose, Auckland**

**Certified Applicator: Building Contractor:**

**Alliance Waterproofing Naylor Love**

**Building Owner/Property Manager:**

1. **Statement of Intent**
   1. This checklist is to be completed by both the Equus Applicator and the Building Contractor, as a step by step record of compliance with both the Equus Specification provided for the contract, and the requirements of the Manufacturer for Warranty.
   2. A copy of this checklist must be forwarded to the nearest Regional Office of Equus Industries Ltd. A Warranty will not be issued by Equus Industries Ltd. without a copy of this Checklist being filed.
2. A copy of this checklist should form part of the Contract Documentation filed with the Property Manager on job completion.
3. **Areas Treated**

The areas to which Membrane is applied are detailed below, with reference to plans (where appropriate).

Areas of below ground tanking-detail reference 4131EB 4.2 / 4.3 / 4.4 and Aguafin 2-KM

1. **Sign Off**

We confirm that all applicable processes listed in Section 4 have been correctly completed and that sign-off on each stage has been made by a person with the authority to do so.

For:

(Building Contractor)

(Signature)

Date: *I I* (Name)

For: (Equus Applicator)

Date: *I I*

(Signature) (Name)

CELEBRATING

**4**

**YEARS**

**AQUAFIN 2-K/M-Checklist And Method Statement**

\* Denotes those processes which must be signed off by the Building Contractor as well.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **No.** | **Process** | **Completed On** | **Building Contractor** | **Equus Contractor** | **Notes** |
| **1.\*** | Ensure all concrete surfaces are cleaned sufficiently for application of **Equus Chevacryl Admix** primer. |  |  |  |  |
| **2.** | Apply **Equus Chevacryl Admix 50/50 primer**  to concrete substrate. |  |  |  |  |
| **3.** | Apply **Equus Epistixx AC primer** to all fer- rous substrate. Allow to cure. |  |  |  |  |
| **4.** | Apply first coat of **Aquafin 2-K/M Plus** by brush or trowel at approx. 2kgs per m2• |  |  |  |  |
| **6.** | Apply an **Equus Schomburg Aquafin 2-K/M Plus** reinforcement bandage to nominated areas-penetrations, concrete to termination bar |  |  |  |  |
| **8.** | Apply second coat of **Aquafin 2-K/M Plus** by brush at approx. 2kgs per m2. |  |  |  |  |
| **9.** | Check for pinholes and touch up as necessary by means of brush. |  |  |  |  |
| **10.** | System to be inspected on completion. |  |  |  |  |

**Equus Industries Ltd**

**PO Box 601**

**Blenheim Phone: 03 578 0214**

**Email:** [**admin@equus.nz**](mailto:admin@equus.nz)

[**www.equus.nz**](http://www.equus.nz/)