**Inspection Checklist –Field Connections Rough in**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Contractor:** |  | | | |  | **IC-E No.** | | |  | |
| **System:** | BMS | | | |  | **Floor:** | | |  | |
| **Panel No:** |  | | | |  | | | |  | |
| Installation in accordance with the Mechanical Services Specification | | | | | | | | | | |
| **Item - Activity** | | | | **Acceptable** | | | | | | **Comment** |
|  | **Yes** | | **No** | | |
| Correct cable used | | | |  |  | |  | | |  |
| Cable Tray or catenary Installed To Specification | | | |  |  | |  | | |  |
| Field wiring roughed in & cable ties cut back | | | |  |  | |  | | |  |
| Mechanical protection used where required | | | |  |  | |  | | |  |
| Penetrations – All penetration sealed in accordance with acoustic / smoke and fire sealing requirements | | | |  |  | |  | | |  |
| End of cable runs looped up and tied up. | | | |  |  | |  | | |  |
| Cable end to end test prior to fit off | | | |  |  | |  | | |  |
|  | | | |  |  | |  | | |  |
|  | | | |  |  | |  | | |  |
|  | | | |  |  | |  | | |  |
|  | | | |  |  | |  | | |  |
|  | | | |  |  | |  | | |  |
|  | | | |  |  | |  | | |  |
| **Inspected by:** | | *Sub-Contractor’s Site Foreman* |  | | | | | Date | |  |
| **Inspected by:** | | *DPA Site Foreman* | Adam Simons | | | | | Date | |  |
| **Comments** | | | | | | If an NCR is raised - # | | | | |
|  | | | | | | Date Closed | | | | |
|  | | | | | | | | | | |
|  | | | | | | | | | | |
|  | | | | | | | | | | |
| **READY FOR HANDOVER TO COMMISSIONING** | | | | | | | | | | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Received by:** | | *DPA Project Manager* | | Date: |
| **Authorised By** | **Site Foreman / Mgr** | | **Client** | **Project Manager** |
|  |  | |  |  |
|  |  | |  |  |