**Inspection Checklist – Electrical Rough In**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Contractor:** |  | | | |  | **IC-E No.** | | |  | |
| **MSSB No:** |  | | | |  | | | |  | |
| Installation generally in accordance with the Mechanical Services Specification | | | | | | | | | | |
| **Item - Activity** | | | | **Acceptable** | | | | | | **Comment** |
|  | **Yes** | | **No** | | |
| Cable Tray and or catenary installed as per specification & earthed | | | |  |  | |  | | |  |
| Seismic restraints installed where required. | | | |  |  | |  | | |  |
| Cables roughed in | | | |  |  | |  | | |  |
| Cable ties cut back | | | |  |  | |  | | |  |
| Cable Type and Size Installed To Specification | | | |  |  | |  | | |  |
| Cable separation has been checked and complies | | | |  |  | |  | | |  |
| All external cable glands fitted and tightened | | | |  |  | |  | | |  |
| Penetrations – All fire and acoustic penetrations have been sealed in accordance with relevant requirements and labelled. | | | |  |  | |  | | |  |
|  | | | |  |  | |  | | |  |
|  | | | |  |  | |  | | |  |
|  | | | |  |  | |  | | |  |
|  | | | |  |  | |  | | |  |
|  | | | |  |  | |  | | |  |
|  | | | |  |  | |  | | |  |
|  | |  |  | | | | |  | |  |
| **Inspected by:** | | *Sub-Contractor’s Site Foreman* |  | | | | | Date | |  |
| **Inspected by:** | | | | | | *DPA Site Foreman* | | | | | Adam Simons | Date | | 27/02/24 |
| **Comments** | | | | | | If an NCR is raised - # | | | | |
|  | | | | | | | | | | | Date Closed | |
|  | | | | | | | | | | |
|  | | | | | | | | | | |
|  | | | | | | | | | | |
| **READY FOR HANDOVER TO COMMISSIONING** | | | | | | | | | | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Received by:** | | *DPA Project Manager* | | Date: |
| **Authorised By** | **Site Foreman / Mgr** | | **Client** | **Project Manager** |
|  |  | |  |  |
|  |  | |  |  |