ITP Façade - Waterproofing

Per block (Only applies to Block A,C & D)

1. Pre-start
   1. Balcony nibs, falls & finish checked
   2. Outlet Flanges installed in correct location
   3. Balustrade Fixings D&E complete
   4. Canopy roof complete & outlets installed
   5. Clean work area
2. Hold point: Council inspection
3. Access/safety/protection
   1. Safe access & Edge protection in place
   2. Hot works permit issued
4. Installation
   1. Waterproofing installed as per drawings
      1. 20mm Fillets installed
      2. Primer installed to substrate
      3. Membrane flashings installed to all corners/penetrations
      4. Metal Grid installed to substrate
      5. Vent sheet applied
      6. Base Sheet installed(Side laps min 100mm , end laps min 150mm)
      7. Capping Sheet Installed(All joints welded & Seamed off)
      8. Danco TD830 tape applied to bifold openings & timber bottom plate
      9. Terminated to blockwork with Protectowrap EIFS tape and no.100 primer
   2. Hold Point: ILD Testing and Remedials Completed
5. Post install
   1. Consultant Inspections & Close Out received
   2. Subcontractor QA received
   3. ILD Report Attached