ITP Façade – Aluminium Joinery

Per block

1. Pre-start
   1. Carpentry sign-off received
   2. HOLD POINT: GN opening size & setout check complete
   3. Clean work area
   4. Weatherline & Flashing Tapes completed
2. Install
   1. Primer applied to hinged/bifold door sills
   2. Window Surround Flashings fixed in place
   3. Frame Installation
      1. Frame installed, PF rod & packers installed
      2. GN Check - Drainage Holes clear from tape protection
      3. Rear Air Seal & fixing sealant complete - Min 6mm sealant gap
   4. Glazing & wedging complete
   5. Surround Flashings sealed
3. Post install
   1. Protection 1.5m high to all doors
   2. HOLD POINT: Façade Engineer Site Inspection Completed
   3. AAMA 501 water test completed and passed – results received
   4. All associated CANs/Inspection Reports are actioned and closed out
   5. Subcontractor QA received