ITP - Fit-out

Per block

1. Pre-start
   1. Lining & Stopping Complete
   2. Hold Point: Council Post Line Inspection Passed where required
   3. Clean Work Area
2. Installation
   1. Tiling and waterproofing
      1. Stopping complete
      2. Waterproofing Installed & QA provided
      3. Tiling & Selants complete & QA provided
   2. Kitchen & Bathroom Cabinetry installed as per the drawings
   3. Services 2nd fix complete
   4. Flooring & Wardrobe Install complete
   5. HWC Nogging & Strapping complete
   6. Services Connection & Commissioning complete
3. Post Installation
   1. Subcontractor QA Received
   2. Council Final Inspection Passed
   3. GN & Architect Defect Inspection Completed