# B!iolytiix Domestic Filter Service Check.hst

10/09/2019

Date of Service:

Job Number:

69584

# Techniic,i.an:

Client Name: Site Ac!clress: Region: Contact Phone: Contact Email:

## Eddie

Stan & Joselyn Ang

44 Millstone Lane, Pokeno, Auckland, 2471

## Auckland

021 886 143

Biolyli:,:: Type:

Filter Seri N1.1mbe1: (9 digits) Alarm Type:

0 Audio-Vrssual {on CBE)

D AUST Manuract1.1recl

D NZ Ma11utac1ured

BF6 3000P

D Audio-Visual (in house)

D Tele111elry

.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Pa" 1 • | | | llnltlal Chook9 | | | | | | | | | *Comment 01 Tick Complete* |
| 1. l' | | nsooct around lank. Are a.II lids inlacl and in olaoe? | | | | | | | | | | ***V***  **a** |
| 2. Take p'.holo ol tank lid, control bo,x eno1osu:re {CB!;) and surrounds? | | | | | | | | | | | |  |
| **Part 2** • **EHIUe:At O.lleck** *(lobe completed before dlslurbif1!} the elfluenl)* | | | | | | | | | | | | |
| 3. Visual (comme11l) I I Odour (comment) | | | | | | | | | | | | ***V*** |
| **Pa:11.3** • **Control Box** & **Filter Bed Olieciks** | | | | | | | | | | | | |
| 4. Take lid oll top ol CBE a.lild confirm internal is dry and clean | | | | | | | | | | | | ***V***  **a** |
| 5. Take a photo of Uie lilter bed (including inlel) | | | | | | | | | | | |  |
| 6 | Commenl on condition of beet any odour and worm ao i\lilY? Flooded | | | | | | | | | | | ***V*** |
| *7.* Remove any | | | | | | .acoumulati;;:d plastics (or non-biodegradatll rnateriaij from the filter bed | | | | | | ***V*** |
| **Part 4** • **Component Ch.eek** | | | | | | | | | | | | |
| 8 | Start pump a11d dheck plumbing fillingsare light Md lhere are no obvious lea'ks | | | | | | | | | | | ***V***  **a** |
| 9. Re111ove 111.1mp. Talle photo of b:iofilm on base | | | | | | | | | | | |  |
| 10, Remove inlake screen and cleat1 pump & floal slVilches thoroughly. Replace inlcrke SGfeen | | | | | | | | | | |  | ***V*** |
| **11.** Float Switches - test alarm float and pump sroplstart float Repl if sticking | | | | | | | | | | | | ***V*** |
| 12, Check localion ol Non Return Val\le (NR:V} felooale ii necessary, Remove, olean & replac:e NRV and Air Valve | | | | | | | | | | | | ***V*** |
| 13, Iii lhere is a lelemetry alaim? If so recommend replacing wilh a visual alarm light moun.ted on Cl8E | | | | | | | | | | | | ***V*** |
| 14. Oleck alarm(s) are operating satisractorily | | | | | | | | | | | | ***V*** |
| **15,** Check lhe alr pump is operaliing satf<sfaotorll)". Check for klnks or leaks In air line or airline fittings | | | | | | | | | | | | ***V*** |
| 16. If auto | | | | , lush va1ves are installed r | | | ,ep!ac:e with a manual il1.1Sh valve al end ol eaoh clripline lalqral | | | | | ***V*** |
| **Part 5** - **lr,igallon System** | | | | | | | | | | | | |
| 17, Visual check • insipec1 all irrigalion areas. Look: lot leaks or areas where e:i:cess water J | | | | | | | | | | 1low has occurred | | ***V*** |
| 18. Activate PufTlp. Open manual flush valv | | | | | | | | ,e{s} in field and oonnect l | .emPQrary flush hose(s) to divert flushing | | | ***V*** |
| water lo land | | | | | | | | | | | |
| 19. Fil a water melel' belween the cam!ock fittings, aclilfale the pump allcl allqr 30 Se(;onds chec:k **lhe** pressurised  flo,w ra!e 01·the- pump in Umin | | | | | | | | | | | | **L/min** |
| **Part 6** - **Final Cheo'k** | | | | | | | | | | | | |
| 20, Ensure unil | | | | | .is switched on | | | | | | | ***V*** |
| 21, Coeck tank, CBE and inspection lids are in pl.ace and secure | | | | | | | | | | | | ***V*** |
| 22, Check all flush valves are ctosed | | | | | | | | | | | | ***V*** |
| 23. E;;nsure sile is tidy belore, leaving | | | | | | | | | | | | ***V*** |
| 24, Comments/Observaltons/Sile Noles:  Non biological substances in system. Pump running hot, showing signs of overheating. Will need follow up | | | | | | | | | | | | |

.

.

Tech Signature:

June 2018