|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **VISUAL INSPECTION REPORT *AS/NZS ISO 17637 —2019 Non-destructive testing—Visual inspection of metal products and components.*** | | | | | | | |
| Client/Job No.: | | | | Report No.: | | | |
| Welding standard: AS/NZS 1554 Part 1 | | | | Weld category: | | | |
| Any specific job requirements: | | | | | | | |
| Stage of fabrication/welding: Before welding – During welding – After welding - | | | | | | | |
| Viewing conditions: Daylight – □ Artificial lighting - (Min. 500 Lux)  Note any access or other restrictions | | | | | | | |
| Surface condition: □ Cleaned of slag, spatter □ Other (state): ................................................................................... | | | | | | | |
| Part/Assy. ID | % inspected  (if less than 100%) | Weld inspection to AS/NZS 1554.1 | Dimensions, tolerances to NZS 3404.1  AS/NZS 5131 | | Any special features, comments | Compliance | |
| C | DNC |
|  |  |  |  | |  |  |  |
|  |  |  |  | |  |  |  |
|  |  |  |  | |  |  |  |
|  |  |  |  | |  |  |  |
|  | | | | | | | |
| Date, place of inspection: | | | | | | | |
| Inspector Signed Date of completed inspection: | | | | | | | |