1. All relevant KCL drawings and revision numbers checked and attached
2. Installation location
3. Timber Frame 800mm x 300mm Steel Studs 300mm x 300mm
4. Correct fasteners used and installed at correct centres
5. Fasteners – 12mm from the edges and 18mm from ends
6. Fasteners – 200mm centres along sheet end butt joints
7. Are screws over driven? If YES, install a new screw fixing 25mm away and adjacent to the over driven screw.
8. Is the GIB installed hard up against the floor.
9. Installer details