|  |  |
| --- | --- |
| Field Inspection Checklist ENTRY TURNOUT | A black and white logo  AI-generated content may be incorrect. FIC Content – Revision A |

| Property/LOCATION: | SITE/Access track id: |
| --- | --- |

| ITEM | | **Checked By:** | | |
| --- | --- | --- | --- | --- |
| RSA | | |
|  | Initial | Date |
| 1 | CH and FDM Clearance | Hold Point |  |  |
| 2 | Set out Entry Turnout dimensions and Delineate Clearance Boundaries | Monitor |  |  |
| 3 | Clear & Grub | Monitor |  |  |
| 4 | Box out if required | Monitor |  |  |
| 5 | Install Invert Table Drain if required | Monitor |  |  |
| 6 | Gravel cap Entry Pavement | Hold Point |  |  |
| 7 | Install Bitumen Two Coat Seal - 14/10mm C170 | Monitor |  |  |
| 8 | As Built Completed | Document |  |  |
| 9 | RSA QA Inspection | Hold Point |  |  |
| **Comments** | | | | |
|  | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Verification of Work Completed:** | | | |
| **RSA Supervisor** | | **Senex Representative** | |
| Name: |  | Name: |  |
| Signature: |  | Signature: |  |
| Date: |  | Date: |  |
| Position: |  | Position: |  |