A black and white logo

AI-generated content may be incorrect.

|  |  |
| --- | --- |
| Field Inspection Checklist Piling | FIC Content – Revision A |

| Property/LOCATION: | SITE/Access track id: |
| --- | --- |

| ITEM | | **Checked By:** | | |
| --- | --- | --- | --- | --- |
| RSA | | |
|  | Initial | Date |
| 1 | Obtain Senex Excavation Permit | Permit Document |  |  |
| 2 | Confirm Set out | Monitor |  |  |
| 3 | Install P3 (control) to 1000mm above ground | Monitor |  |  |
| 4 | Drive P1, P2 and all remaining Piles to correspond with the control (P3) | Monitor |  |  |
| 5 | Tug test to client specification to be completed on at minimum two Piles. | Monitor |  |  |
| 6 | Confirm all Piling Height and Final Location measurements are correct within client specification & Control (P3) | Measure |  |  |
| 7 | As Built Completed | Document |  |  |
| 8 | RSA supervisor inspection | Hold point |  |  |
| **Comments** | | | | |
|  | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Verification of Work Completed:** | | | |
| **RSA Supervisor** | | **Senex Representative** | |
| Name: |  | Name: |  |
| Signature: |  | Signature: |  |
| Date: |  | Date: |  |
| Position: |  | Position: |  |