A black and white logo

AI-generated content may be incorrect.

|  |  |
| --- | --- |
| Field Inspection Checklist LEASE PADS | FIC Content – Revision 0 |

| Property/LOCATION: | SITE/Access track id: |
| --- | --- |

| ITEM | | **Checked By:** | | |
| --- | --- | --- | --- | --- |
| RSA | | |
|  | Initial | Date |
| 1 | CH and FDM clearance | Hold Point |  |  |
| 2 | Identify work area, boundaries and survey requirement | Monitor |  |  |
| 3 | Evenly spread DAP fertilizer onto the topsoil prior to stripping | Monitor |  |  |
| 4 | Clear & Grub Topsoil and stack timber | Monitor |  |  |
| 5 | Lease Entry Construction | Monitor |  |  |
| 6 | Lease construction | Monitor |  |  |
| 7 | Compaction of layers in 300mm layers | Monitor |  |  |
| 8 | Proof roll | Monitor |  |  |
| 9 | Verification of cross falls/laser set ups | Monitor |  |  |
| 10 | Final Trim | Hold Point |  |  |
| 11 | DCP Testing | Witness |  |  |
| 12 | Gravel Cap (as required) | Monitor |  |  |
| 13 | Install ESC | Monitor |  |  |
| 14 | Cellar Installation | Monitor |  |  |
| 15 | Conductor Installation – Record plumb | Monitor |  |  |
| 16 | Conductor cemented in place | Monitor |  |  |
| 17 | 4 x cattle panels to be installed | Monitor |  |  |
| 18 | Well signage and Pipeline entry mark completed | N/A |  |  |
| 19 | As Built Completed | Monitor |  |  |
| 20 | RSA supervisor inspection | Hold point |  |  |
| **Comments** | | | | |
|  | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Verification of Work Completed:** | | | |
| **RSA Supervisor** | | **Senex Representative** | |
| Name: |  | Name: |  |
| Signature: |  | Signature: |  |
| Date: |  | Date: |  |
| Position: |  | Position: |  |