**Inspection and test plan – Concrete Pile Cropping**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Project no.** | | CC0398 | | | **Project name** | VIVA Energy ULSG | | | | | **Date** | |  | | **Approved by** |  |
| **ITP no.** | 3 | | | | **Revision no.** | A | **Revision date** | | 25/10/2023 | **Plant and equipment used** | | | |  | | |
| **Lot no.** |  | | | | **Location (chainages, detailed description or marked up plan)** | | | | | | |  | | | | |
| **Layer thickness** | | |  | **Estimated qty** | |  | |

Attach Dockets, Certificates and QA Documents to ITP

|  | |  |  |  |  | **Verification or test by** | | | | | **Remarks / record (eg. test frequency, reports, certificates, checklist etc)** | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  |  |  |  | **Symal Infrastructure** | | | **MCR** | |
| **Item no.** | | **Activity** | **Ref docs** | **Acceptance criteria** | **Frequency** | **Key** | **Resp.** | **Initial/date** | **Key** | **Sign date** |
| **1.0 Preliminaries** | | | | | | | | | | | | |
| **1.1** | | Starter Bars |  | Are starter bars (if exposed) in suitable condition:   * Straight * Free from excessive rust * Correct height projections   ☐ Yes ☐ No ☐ N/A | Once per Pile | S |  |  |  |  |  | |
| **2.0 Pile Cropping** | | | | | | | | | | | | |
| **2.1** | | Set out | DWG No. GRN-92002-030002 – 10 | Pile cut off has been marked by survey  ☐ Yes ☐ No ☐ N/A | Once per pile | W |  |  |  |  |  | |
| **2.2** | | Pre-Cutting (if required) |  | Has the pile been pre-cut along survey marked level i.e. ring cut method  ☐ Yes ☐ No ☐ N/A | Once per pile | S |  |  |  |  |  | |
| **2.3** | | Irregular Concrete |  | Large uneven/jagged concrete sections to be removed to create flat concrete cut off level | Once per pile | S |  |  |  |  |  | |
| **3.0 Conformance check** | | | | | | | | | | | | |
| **3.1** | | Tolerance | DWG No. GRN-92002-030002 – 10  As per civil (235929) drawings | Survey to check actual pile cut off level is within +-+-25mm of cut off level.  ☐ Yes ☐ No ☐ N/A | Once per pile | S |  |  |  |  |  | |
| **3.2** | | As Builts |  | Survey to pick up cut off levels for as-builts  ☐ Yes ☐ No ☐ N/A | Once per pile | S |  |  |  |  |  | |
|  | **Comments:** | | | | | | | | | | |  |
|  |  | | | | | | | | | | |  |
|  |  | | | | | | | | | | |  |
|  |  | | | | | | | | | | |  |
|  |  | | | | | | | | | | |  |
|  |  | | | | | | | | | | |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Lot acceptance:** | | | | |
| Symal Infrastructure representative name |  |  | Client representative name |  |
| Symal Infrastructure representative signature |  |  | Client representative signature |  |