|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ACTIVITY DESCRIPTION | STEP | INSPECTION FUNCTION | APPLICABLE STANDARD | ACCEPTANCE CRITERIA | SWMS | VAST INSPECTION | SIGNATURE | DATE | RECORDS/ REMARKS RESULTS |
| DELIVERY CHECK FOR DAMAGE | 1 | VISUAL | NO DAMAGE | COMPLIES |  |  |  |  |  |
| INSTALL HARD WIRING TERMINATION POINT | 2 | CHECK FIXINGS | AS/NZS  3000:2007 | MANUFACT. RECOMMEND-ATIONS |  |  |  |  |  |
| TERMINATE CABLE AT TERMINATION BOX | 3 | CORRECT TERMINATION POINT CONNECTIONS TIGHT | AS SPEC | CONNECTION CORRECT HAND TIGHT |  |  |  |  |  |
| LOOP FLEXIBLE LEAD FROM TERMINATION BOX TO LIGHT SWITCH, SENSOR OR OUTLET AS REQUIRED | 4 | CHECK CONNECTORS | AS/NZS  3000:2007  ELEC/DRWG | CHECK CONNECTOR MATED CORRECTLY |  |  |  |  |  |
| TEST AND COMMISSION | 5 | INSPECTION | AS/NZS  3000:2007 | COMPLIES WITH REGS |  |  |  |  |  |