|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ACTIVITY DESCRIPTION | STEP | INSPECTION FUNCTION | APPLICABLE STANDARD | ACCEPTANCE CRITERIA | SWMS | VAST INSPECTION | SIGNATURE | DATE | RECORDS/ REMARKS/RESULTS |
| OBTAIN THE MOST RECENT DRAWINGS AND SPECIFICATIONS. | 1 | CHECK | DRAWING REGISTER | CORRECT DRAWINGS |  |  |  |  |  |
| INSTALL CABLE SUPPORT OR CONDUIT WHERE REQUIRED. | 2 | CHECK FIXING | SPEC. & DRAWING  AS/ACIF 3009:2006  AS/ZS 3080, AS/NZS 3034 | COMPLIES |  |  |  |  |  |
| DRESS CABLES TO FINAL LOCATION. ENSURE VELCRO STRAPS FOR CAT 6 CABLING | 3 | CHECK | DRAWINGS & SPEC. | COMPLIES |  |  |  |  |  |
| TERMINATE CABLING ENSURING CORRECT COLOUR CODE. ensure correct termination tool used as per vendor recommendation | 4 | CHECK TERMINATIONS | AS/ACIF 3009:2006  AS/ZS 3080, AS/NZS 3034 | COMPLIES |  |  |  |  |  |
| test terminations using wizard tester for krone block terminations and mod tap tester for patch panel terminations.  device number: | 5 | TEST | AS/ACIF 3009:2006  AS/ZS 3080, AS/NZS 3034 | COMPLIES |  |  |  |  |  |
| LABEL FRAMES AND COMPLETE RECORD BOOKS | 6 | LABELLING | AS/NZS 3085.1 : 2004 | COMPLIES |  |  |  |  |  |
| RECORD RESULT | 7 | RESULTS | AS/ACIF 3009:2006  AS/ZS 3080, AS/NZS 3034 | COMPLIES |  |  |  |  |  |
| COMPLETE TELECOMMUNICATIONS CABLING ADVICE FORM AND ATTACHMENT IF REQUIRED | 8 | TELECOMMUNICATIONS ADVICE | AS/acif s009:2006 | COMPLIES |  |  |  |  |  |