|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ACTIVITY DESCRIPTION | STEP | INSPECTION FUNCTION | APPLICABLE STANDARD | ACCEPTANCE CRITERIA | SWMS | VAST INSPECTION | SIGNATURE | DATE | RECORDS/ REMARKS/RESULTS |
| OBTAIN THE RELEVANT AND MOST RECENT DRAWINGS AND SPECIFICATION. | 1 | CHECK | DRAWING REGISTER | DRAWING REGISTER |  |  |  |  |  |
| INSTALL CABLE SUPPORT OR CONDUIT WHERE REQUIRED. | 2 | CHECK FIXINGS | AS 3080, SPEC. & DRAWING  AS 3000 | COMPLIES |  |  |  |  |  |
| VERIFY CORRECT CABLE TYPE. | 3 | CHECK | DRAWINGS & SPEC. | COMPLIES |  |  |  |  |  |
| DECIDE APPROPRIATE CABLE NUMBERING SEQUENCE RELEVANT TO FINAL FIT OFF SEQUENCE. | 4 | RECORD DETAILS | LEGIBLE & CAN BE FOLLOWED BY OTHERS. | COMPLIES |  |  |  |  |  |
| INSTALL CABLE WITHIN OR ON CABLE SUPPORT SYSTEM AS APPROPRIATE. | 5 | VISUAL | AS 3080, SPEC. & DRAWING  AS 3000 | COMPLIES |  |  |  |  |  |
| FORM CABLES INTO RELEVANT FIT-OFF GROUPS AT THE CABINET END. | 6 | VISUAL | NEAT & TIDY | COMPLIES |  |  |  |  |  |