|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ACTIVITY DESCRIPTION | STEP | INSPECTION FUNCTION | APPLICABLE STANDARD | ACCEPTANCE CRITERIA | SWMS | VAST INSPECTION | SIGNATURE | DATE | RECORDS/ REMARKS RESULTS |
| VISUAL CHECK ENSURING CABLE TO BE FITTED OFF IN CORRECT POSITION. | 1 | VISUAL | DRAWING & SPEC. | COMPLIES |  |  |  |  |  |
| SELECTION OF CORRECT TOOL TO BE USED FOR TERMINATION TYPE. | 2 | CHECK | MANUFACTURER RECOMMENDATION |  |  |  |  |  |  |
| INSTALL PATCH PANEL INTO CABINET LOOM CABLES TO THE BACK OF THE PATCH PANEL. TIE INTO POSITION USING VELCRO STRIP AND/OR CABLE TIES SUPPLIED. | 3 | CHECK | AS 3080 & MANUFACT. REQUIREMENTS | COMPLIES |  |  |  |  |  |
| ENSURE CABLES ARE STRIPPED NO MORE THAN THE SPECIFIED DISTANCE. CHECK TERMINATIONS AT COMPLETION FOR COLOUR CODE AND SEQUENCE. | 4 | CHECK | AS 3080 & MANUFACT. REQUIREMENTS | COMPLIES |  |  |  |  |  |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ACTIVITY DESCRIPTION | STEP | INSPECTION FUNCTION | APPLICABLE STANDARD | ACCEPTANCE CRITERIA | JSA/SWMS | VAST INSPECTION | SIGNATURE | DATE | RECORDS/ REMARKS RESULTS |
| ATTACH WRAP AROUND LABEL TO CABLE NO MORE THAN 60MM FROM THE JACK. ENSURING CORRECT NUMBER SEQUENCE. | 5 | CHECK | DRAWINGS & SEPC. | COMPLIES |  |  |  |  |  |
| INSTALL PATCH PANEL INTO EQUIPMENT RACK OR CABINET. | 6 | CHECK. | DRAWINGS & SEPC. | COMPLIES |  |  |  |  |  |
| LABEL OUTLET ENSURING CORRECT NUMBER SEQUENCE | 7 | ENSURE CORRECT LABEL TYPE. | DRAWINGS & SEPC. | COMPLIES |  |  |  |  |  |