**We Build Foundations Pty Ltd**

PO BOX 3011

Balgownie, New South Wales 2519 P: 0407-421-255

Inspection: Framing Carpentry #2

**Project: MH-0002 9 Point Street Bulli**

9 Point Street Bulli, New South Wales 2516

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **0/9**  Items Inspected |  | **0**  Conforming |  | **0**  Deficient |  | **0**  N/A |  | **0**  Neutral |

|  |  |  |  |
| --- | --- | --- | --- |
| **Type** | Commissioning | **Status** | Open |
| **Trade** | Carpenter | **Location** | 9 Point Street |
| **Spec Section** |  | **Created By** | Angelica Borja |
| **Linked Drawings** |  |  |  |

**Description** Ensure structural integrity, compliance with engineering designs, and adherence to safety standards during the installation process.

**Attachments** [ITP\_Framing Carpentry.pdf](https://storage.procore.com/v4/d/ap-southeast-2/prostore-apse2/companies/832115523431895/01J1VN0GZPJ8Z07H5H4CQEH2Y7?sig=300489093f58c1da499fbe6427a892ef7ff72a8610085996a15bae7cbc4a9798)

**Inspection Details**

**Inspection Date Due Date**

**Point of Contact Responsible**

**Contractor**

**Assignee(s)** Angelica Borja

**Install wall frames 0 Neutral 0 Conforming 0 Deficient 0 N/A**



**1.1 Check that all wall frames are plumb, level, and square.**

Details: Australian standard for Frames and Trusses Carpentry

Pass

Fail

N/A



**1.2 Verify that fasteners are properly placed and secure.**

Details: Australian standard for Frames and Trusses Carpentry

Pass

Fail

N/A



**1.3 Ensure openings for doors and windows are correctly framed.**

Details: Australian standard for Frames and Trusses Carpentry

Pass

Fail

N/A

**Inspect roof trusses 0 Neutral 0 Conforming 0 Deficient 0 N/A**



**2.1 Confirm that trusses are installed according to the design plan.**

Details: Australian standard for Frames and Trusses Carpentry

Pass

Fail

N/A

**Inspection #2 - Framing Carpentry Project: MH-0002 9 Point Street Bulli**



**2.2 Check for proper bracing and connections at all joints.**

Details: Australian standard for Frames and Trusses Carpentry

Pass

Fail

N/A



**2.3 Verify that trusses are not damaged and are aligned correctly.**

Details: Australian standard for Frames and Trusses Carpentry

Pass

Fail

N/A

**Test structural integrity 0 Neutral 0 Conforming 0 Deficient 0 N/A**



**3.1 Inspect for any signs of warping, bowing, or movement in the frame.**

Details: Australian standard for Frames and Trusses Carpentry

Pass

Fail

N/A



**3.2 . Ensure that load-bearing elements are correctly supported**

Details: Australian standard for Frames and Trusses Carpentry

Pass

Fail

N/A



**3.3 Confirm that all structural elements meet safety and design standards.**

Details: Australian standard for Frames and Trusses Carpentry

Pass

Fail

N/A