***6-8 Munroe Lane QA addition. ZYJ construction.***

Name of list.

**-Level 3 balustrade framing.**

Locations.

**-East elevation**

**-West elevation**

**Set out check list.**

**-**previous trade QA received

-set out matches TCL drawings

- set out in within tolerance of TCL flashings

-R/L tolerance in accordance with TCL and structural steel.

-up to date plans on site.

**Framing checklist.**

-to plate and bottom plate fixed in accordance with details.

-Framing set to grid lines

-R/L in accordance with plans

-studs at 600c

-plywood fixed off in accordance with specification

-cap flashing packing to specified fall

- cap flashing packing set to TCL R/L

-cap flashing packing set out with in tolerance for under flashings

-plywood fixed off in accordance with specification