|  |  |  |  |
| --- | --- | --- | --- |
| Type | Description | Complete | ITR - Ref |
| General Lighting - Internal | 4 x 5ft LED Light Fitting |  | PFI-ITR-0103 |
| General Lighting - Internal | 2 x 90deg PIR Sensor (internal lighting) |  | PFI-ITR-0103 |
| General Lighting - External | 2 x LED External Bulkhead Light Fitting |  | PFI-ITR-0104 |
| General Lighting - Emergency Internal | 2 x 5ft LED Emergency Light Fitting |  | PFI-ITR-0103 |
| General Lighting - Emergency Internal | 2 x Illuminated EXIT light fitting with Batt backup |  | PFI-ITR-0103 |
| General Electrical - GPO | 2 x Double 10A 1ø Switched Socket Outlet |  | PFI-ITR-0100 |
| General Electrical - GPO | 2 x Double 10A 1ø UPS Protected Red Switched Socket Outlet |  | PFI-ITR-0100 |
| General Electrical - GPO | 1 x 15A 1ø Weatherproof Exterior Switched Socket Outlet |  | PFI-ITR-0100 |
| General Electrical - GPO | 1 x 32A 3ø Weatherproof Exterior Switched Socket Outlet |  | PFI-ITR-0100 |
| General Lighting - Switch | 2 x Two-Way Two-Gang Switch |  | PFI-ITR-0103 |
| General Lighting - Switch | 1 x Auto-Off-Manual Switch |  | PFI-ITR-0103 |