|  |
| --- |
| **Type** |
| checklist |
| checkpoint |
| button |
| button |
| button |
| button |
| button |
| button |
| button |
| button |
| button |
| button |
| signoff |
| signoff |

|  |  |
| --- | --- |
| **Name** | **Values** |
| Fibre/Comms Duct |  |
| Fibre/Comms Duct |  |
| Duct is installed as per drawings | Yes,N/A |
| Frame identification marked correctly and visible. | Yes,N/A |
| Duct is free from damage | Yes,N/A |
| Duct is sufficiently supported | Yes,N/A |
| Ducting is connected properly | Yes,N/A |
| Tubing is correctly fitted into cabinet entries | Yes,N/A |
| Lid is installed | Yes,N/A |
| Cables entering and leaving transits adequately supported and protected. | Yes,N/A |
| Cables pass through frames without strain on duct | Yes,N/A |
| As-builts complete. | Yes,N/A |
| Installed by: |  |
| Add applicable signatures (e.g Electrician, Inspector, Client Representative) |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Prefix** | **Postfix** | **Usage**  **Count** | **User**  **Addable** | **Template**  **Name** |
|  | | | | |