

# Attention: Lockwood Flooring

1/8 Vella Drive

Sunshine West VIC 3012

# Project Name: Footscray Hospital Commercial Building D

Builder: Multiplex

Installer: Lockwood Flooring Australia Pty Ltd

**Sign**

**Date**

**Pass**

**Complete**

**Task**

VINYL - INSPECTION TEST PLAN

Working to latest plan revisions and check latest correspondence

1. Prior works checks   Area free of building debris and trade tools   Walls plastered and first coat of paint  

1

All adjacent finishes completed and ready to receive finishes. Area to be flagged if LF cannot finish 100%

1.  Specification checks - Correct materials as per finishes schedule and sample approvals
2.  Installation procedure as per manufactures recommendations and AUS standards -

Barridcaded areas   Grind, vac and clean   Apply moisture barrier as required  

Prime and self level as quoted (3mm)  

Set out vinyl to minimise waste and cross joins

Apply cove fillet to perimeter as required   Install vinyl and cove with recommended

adhesive

Heavy roll finished floor  

1. Protection - corflute plastic  
2. Confirm material warranty applies  
3.  Confirm installation warranty 12 months applies
4. Care and maintenance as per O&Ms





**Level Area Complete Pass Date Sign Notes**