

# Attention: Lockwood Flooring

1/8 Vella Drive, Sunshine West VIC 3012

# Project Name: Victoria University Building E

Builder: Multiplex

Installer: Lockwood Flooring Australia Pty Ltd

Timber - INSPECTION TEST PLAN

**Task Complete Pass Date**

Working to latest plan revisions and check latest correspondence

1

2 Prior works checks   Area free of building debris and trade tools   Walls plastered and first coat of paint  

All adjacent finishes completed and ready to be finishes. Area to be flagged if LF cannot finish 100%

Specification checks - Correct materials as per finishes schedule and sample approvals

3

1.  Installation procedure as per manufactures recommendations and AUS standards -

Barridcaded areas   Vac and clean area  

Floor prep (grind, MB, 3mm) as required   Ensure joinery kickers, skirting boards etc removed

where possible

Set out Rezil sleeper system as per manufacturer recommendations

Set out solid timber to sleepers   Install timber with recommended adhesive and

secret nails

Allow for expansion gaps at perimeter and to fixtures   Sand and seal timber as per manufacturer

recommendations

1. Protection - corflute plastic  
2. Confirm material warranty applies  
3. Confirm installation warranty 12 months applies



8

Care and maintenance as per O&Ms

Lockwood Flooring **|** 1/8 Vella Drive, Sunshine West VIC 3020 **| lockwoodflooring.com.au**



**Level Area Complete Pass Date Sign Notes**

 



Lockwood Flooring **|** 1/8 Vella Drive, Sunshine West VIC 3020 **| lockwoodflooring.com.au**