A black and white logo

AI-generated content may be incorrect.

|  |  |
| --- | --- |
| Field Inspection Checklist fENCING & GRIDS | FIC Content – Revision A |

| Property/LOCATION: | SITE/Grid ID: |
| --- | --- |

| ITEM | | **Checked By:** | | |
| --- | --- | --- | --- | --- |
| RSA | | |
|  | Initial | Date |
| 1 | CH & FDM Clearance | Hold Point |  |  |
| 2 | Identify Work Area, boundaries of Fencing | Monitor |  |  |
| 3 | Inspect fencing materials | Monitor |  |  |
| 4 | Installation of fencing | Monitor |  |  |
| 5 | Concrete for base of fencing | Monitor |  |  |
| 6 | Fence posts caps | Monitor |  |  |
| 7 | Welding | Monitor |  |  |
| 8 | Galvanized Painting at Welds | Monitor |  |  |
| 9 | Gate Chain and Carabiner Clips | Monitor |  |  |
| 10 | Box Out Grid Footings and Prep Site | Monitor |  |  |
| 11 | Inspect grid materials | Monitor |  |  |
| 12 | Compaction for Grid base | Monitor |  |  |
| 13 | Concrete Abutment / Install Base Slab (if required) | Monitor |  |  |
| 14 | Position and Install Grid | Monitor |  |  |
| 15 | Install and Compact Gravel Ramps | Monitor |  |  |
| 16 | Attach Fence to Box Assembly | Monitor |  |  |
| 17 | RSA QA inspection | Hold Point |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Verification of Work Completed:** | | | |
| **RSA Supervisor** | | **Senex Representative** | |
| Name: |  | Name: |  |
| Signature: |  | Signature: |  |
| Date: |  | Date: |  |
| Position: |  | Position: |  |

|  |
| --- |
| **Comments** |
|  |