|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ACTIVITY DESCRIPTION | STEP | INSPECTION FUNCTION | APPLICABLE STANDARD | ACCEPTANCE CRITERIA | SWMS | VAST INSPECTION | SIGNATURE | DATE | RECORDS/ REMARKS RESULTS |
| VISUAL CHECK OF OUTLETS FOR COMPLETION. | 1 | VISUAL | AS/NZS 3080:2003 | COMPLIES |  |  |  |  |  |
| SELECTION OF CORRECT TESTING INSTRUMENT.  TEST DEVICE NUMBER: …………………… | 2 | VISUAL | AS/NZS 3080:2003: | COMPLIES |  |  |  |  |  |
| SELECTION OF CORRECT SETTINGS FOR TEST INSTRUMENTS.  - CABLE TYPE  - OUTLET TYPE  - TERMINATION SEQUENCE  - VENDOR CABLING SPECIFICATIONS  - CORRECT AND SEQUENTIAL PROJECT DETAILS | 3 | CHECK SETTINGS | AS/NZS 3080:2003: | COMPLIES |  |  |  |  |  |
| TEST OUTLETS AND RECORD TEST RESULTS AS SPECIFIED AND/OR REQUESTED | 4 | TEST & RECORD | AS/NZS 3080:2003 | COMPLIES |  |  |  |  |  |
| COMPLETE TELECOMMUNICATIONS CABLING ADVICE FORM AND ATTACHMENT IF REQUIRED | 5 | TELECOMMUNICATIONS ADVICE | AS/acif s009:2006 | COMPLIES |  |  |  |  |  |